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Detailed Technical Requirements for LACNIC Events

Generally speaking, an Internet connection of at least 1 Gbps will be required. A backup link of the same capacity, preferably with another provider to be used as a backup, will be considered a plus.

[bookmark: _GoBack]The Internet link to be used by event participants must be separate from the Internet access link used by the hotel or event venue. The wireless network normally used by the hotel must be disabled in all areas covered by the wireless network set up for LACNIC.

1. Connectivity Detail 

· Symmetrical Internet connection of at least 1 Gbps supporting IPv4 and native IPv6, as well as a backup link of similar characteristics from a different provider.
· Providing connectivity to the hotel rooms used by event participants with the same SSIDs announced in the areas where the event is taking place and through the same link hired for the conference rooms will be considered a plus.
· Public addressing (both IPv4 and IPv6) is required for the entire network. Network translation technologies (NAT) and packet filtering are not allowed.
· Transit for LACNIC's IP prefixes (IPv4 and IPv6) via BGP.
· LACNIC has IPv4 and IPv6 prefixes, as well as an Autonomous System Number:
· IPv4: 45.6.248.0/21 and 200.0.86.0/23
· IPv6: 2001:13c7:7003::/48
· ASN: 28002
· Announcements must be made from the event network, not anchored to the provider's network. The origin AS must be 28002.

2. Infrastructure

· Uninterruptible power supply (UPS)
· Requirements include a UPS properly sized to support potential power outages affecting the equipment installed for the event. This equipment includes the two servers, routers, switches, access points and any additional devices required for the normal provision of network services.

3. Services

· Permanent contact with the connectivity providers' technical support staff. Their contact information (telephone, cell phone, email) must be provided.
· A technical point-of-contact must be available on-site to provide infrastructure and connectivity support. 
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